% Copyright 2018-2023 by Romano Giannetti
% Copyright 2015-2023 by Stefan Lindner
% Copyright 2013-2023 by Stefan Erhardt
% Copyright 2007-2023 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the files gpl-3.0_license.txt and lppl-1-3c_license.txt for more details.

\def\pgfcircversion{1.6.1}
\def\pgfcircversiondate{2023/02/11}
\writestatus{loading}{\pgfcircversiondate{} The CircuiTikz circuit drawing package version \pgfcircversion}

\usemodule[tikz]

\startmodule[circuitikz]
\usetikzlibrary[calc]
\usetikzlibrary[arrows.meta, bending]
\usetikzlibrary[fpu] % may be needed for use fpu reciprocal (v1.0.1)

\unprotect

\edef\tikzatcode{\the\catcode`\@}
\edef\tikzbarcode{\the\catcode`\|}
\edef\tikzexclaimcode{\the\catcode`\!}
\catcode`\@=11
\catcode`\|=12
\catcode`\!=12

\input pgfcirc.defines.tex
\input pgfcircutils.tex
\input pgfcircpath.tex

\input pgfcircshapes.tex
\input pgfcircmonopoles.tex
\input pgfcircbipoles.tex
\input pgfcirctripoles.tex
\input pgfcircquadpoles.tex
\input pgfcircmultipoles.tex

\input pgfcirclabel.tex
\input pgfcircvoltage.tex
\input pgfcirccurrent.tex
\input pgfcircflow.tex

% defaults

\setupmodule
   [current=european,
    voltage=european,
    resistor=american,
    inductor=cute,
    logic=american,
    siunitx=true,
    arrowmos=false]

\processaction
   [\currentmoduleparameter{voltage}]
   [european=>\ctikzset{voltage=european},
    american=>\ctikzset{voltage=american}]

\processaction
   [\currentmoduleparameter{current}]
   [european=>\ctikzset{ current=european},
    american=>\ctikzset{ current=american}]

\processaction
   [\currentmoduleparameter{label}]
   [straight=>\ctikzset{label/align = straight},
    align=>\ctikzset{label/align = rotate},
    smart=>\ctikzset{label/align = smart}]

\processaction
   [\currentmoduleparameter{resistor}]
   [european=>\ctikzset{ resistor=european},
    american=>\ctikzset{ resistor=american}]

\processaction
   [\currentmoduleparameter{inductor}]
   [european=>\ctikzset{ inductor=european},
    american=>\ctikzset{ inductor=american},
    cute=>\ctikzset{ inductor=cute}]

\processaction
   [\currentmoduleparameter{diode}]
   [full=>\ctikzset{ diode=full},
    empty=>\ctikzset{ diode=empty}]

\processaction
   [\currentmoduleparameter{logic}]
   [european=>\ctikzset{ logic ports=european},
    american=>\ctikzset{ logic ports=american}]

\processaction
   [\currentmoduleparameter{siunitx}]
   [true=>\def\SI#1#2{#1\,#2}
    \def\ampere{\rm{A}}
    \def\volt{\rm{V}}
    \def\ohm{\Omega}
    \def\siemens{\rm{S}}
    \def\farad{\rm{F}}
    \def\henry{\rm{H}}
    \def\second{\rm{s}}
    \def\coulomb{\rm{C}}
    \def\siemens{\rm{S}}
    \def\radians{\rm{rad}}
    \def\milli{\rm{m}}
    \def\micro{\mu}
    \def\nano{\rm{n}}
    \def\pico{\rm{p}}
    \def\kilo{\rm{k}}
    \def\mega{\rm{M}}
    \def\giga{\rm{G}}
    \def\tera{\rm{T}},
    false=>]
%   \s!default=>\pgf@circ@siunitxtrue,

\processaction
   [\currentmoduleparameter{arrowmos}]
   [true=>\pgf@circuit@mos@arrowstrue,
    false=>\pgf@circuit@mos@arrowsfalse]
%   \s!default=>\pgf@circuit@mos@arrowstrue,


\ifpgf@circ@siunitx
 % nothing! siunitx and xstrings don't work in context
\fi


% Context specific

\ctikzset{tripoles/op amp/font/.initial=\switchtobodyfont[small]}


\catcode`\@=\tikzatcode
\catcode`\|=\tikzbarcode
\catcode`\!=\tikzexclaimcode

% define the environment
\long\def\startcircuitikz#1\stopcircuitikz{\starttikzpicture#1\stoptikzpicture}

\protect

\stopmodule

\endinput
